{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Chuchu"],"not_rendered":{"charts":0,"images":7,"macros":1,"external_links":0,"defined_names":11,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Chuchu","index":0,"n_rows":35,"n_cols":19,"rows_kept":35,"cut":false,"hidden":false,"merged":[[5,7,5,10],[4,13,4,15],[0,5,0,11],[2,7,2,10],[3,7,3,10],[4,7,4,10]]}
[null,null,null,null,null,"Berekening drukverlies"]
[]
[null,"Type gaz",null,null,"Gaz naturel H",null,"Referenties project",null,null,null,null,null,"Sprache/Language"]
[]
[null,"Temperatuur gas (°C)",null,null,"15","°C"]
[null,"Druk bij aansluiting (Pa)",null,null,"2000","Pa"]
[null,"Toegelaten drukverlies (Pa)",null,null,"300","Pa",null,""]
[null,"Calorische waarde (kWh/m3)",null,null,"10,6","kWh/m³"]
[]
[]
[null,"Lijn","Volgende aansluiting","Volgende aansluiting (Lijn 1)","Volgende aansluiting  (Lijn 2)","Nominale belasting (kW)","Hoogteverschil (m)","Nominale breedte (DN)","T Koppeling","Lengte (m)","90° bocht (aantal)","Aantal koppelingen","Stuk van klant, drukverlies gas (Pa)","Opmerkingen","Drukverlies op de lijn (Pa)","Totaal drukverlies (Pa)"]
[null,"Aanvoer",null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"deutsch"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"english"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"français"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"italiano"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nederlands"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null," ",null,null,null,null,null," "]